Copyright © 2001 - 2002 SILC Project SILC Project Website | SILC Toolkit Reference Manual Index

SILC Toolkit Reference Manual SILC Core Library SILC Authentication Interface SILC Message Interface SILC Channel Interface SILC Command Interface SILC Notify Interface SILC Status Types SILC Modes SILC ID Interface SILC ID Cache Interface SILC Argument Interface SILC Attributes Interface Packet Protocol Interface SILC Math Library SILC MP Interface SILC Math Interface SILC SFTP Library SILC SFTP Interface SFTP Filesystems Interface SILC Utility Library Basic SILC Types SILC Buffer Interface SILC Buffer Format Interface SILC Hash Table Interface SILC Logging Interface SILC Memory Interface SILC Mutex Interface SILC Thread Interface SILC Network Interface SILC Schedule Interface SILC Socket Interface SILC Protocol Interface SILC Config Interface SILC File Util Interface SILC String Util Interface SILC Util Interface SILC List Interface SILC Dynamic List Interface SILC VCard Interface SILC Application Utilities SILC Key Exchange Library SILC SKE Interface SKE Status Types SKE Diffie Hellman Groups SKE Payloads SILC Client Library Using SILC Client Library Tutorial Arguments for command_reply Client Operation SilcStatus Error Arguments in command_reply Client Operation Arguments for notify Client Operation Client Library Interface Reference SILC Crypto Library Introduction to SILC RNG SILC RNG Interface SILC Cipher API SILC PKCS API SILC PKCS#1 API SILC Hash Interface SILC HMAC Interface Resource Links SILC Project Website SILC Protocol Documentation SILC White Paper SILC FAQs
Function silc_command_payload_encode_va SYNOPSIS
        SilcBuffer silc_command_payload_encode_va(SilcCommand cmd,
                                                  SilcUInt16 ident,
                                                  SilcUInt32 argc, ...);
DESCRIPTION
        Encodes Command payload with variable argument list. The arguments
        must be: SilcUInt32, unsigned char *, unsigned int, ... One
        {SilcUInt32, unsigned char * and unsigned int} forms one argument,
        thus `argc' in case when sending one {SilcUInt32, unsigned char *
        and SilcUInt32} equals one (1) and when sending two of those it
        equals two (2), and so on. This has to be preserved or bad things
        will happen. The variable arguments is: {type, data, data_len}.
SILC Command Interface SilcCommandCb SilcCommandPayload SilcCommandFlags SilcCommand silc_command_payload_parse silc_command_payload_encode silc_command_payload_encode_payload silc_command_payload_encode_va silc_command_payload_encode_vap silc_command_reply_payload_encode_va silc_command_reply_payload_encode_vap silc_command_free silc_command_get silc_command_get_args silc_command_get_ident silc_command_get_status silc_command_set_ident silc_command_set_command

Copyright © 2001 - 2002 SILC Project SILC Project Website | SILC Toolkit Reference Manual Index