Copyright © 2001 - 2002 SILC Project SILC Project Website | SILC Toolkit Reference Manual Index

SILC Toolkit Reference Manual SILC Core Library SILC Authentication Interface SILC Message Interface SILC Channel Interface SILC Command Interface SILC Notify Interface SILC Status Types SILC Modes SILC ID Interface SILC ID Cache Interface SILC Argument Interface SILC Attributes Interface Packet Protocol Interface SILC Math Library SILC MP Interface SILC Math Interface SILC SFTP Library SILC SFTP Interface SFTP Filesystems Interface SILC Utility Library Basic SILC Types SILC Buffer Interface SILC Buffer Format Interface SILC Hash Table Interface SILC Logging Interface SILC Memory Interface SILC Mutex Interface SILC Thread Interface SILC Network Interface SILC Schedule Interface SILC Socket Interface SILC Protocol Interface SILC Config Interface SILC File Util Interface SILC String Util Interface SILC Util Interface SILC List Interface SILC Dynamic List Interface SILC VCard Interface SILC Application Utilities SILC Key Exchange Library SILC SKE Interface SKE Status Types SKE Diffie Hellman Groups SKE Payloads SILC Client Library Using SILC Client Library Tutorial Arguments for command_reply Client Operation Arguments for notify Client Operation Client Library Interface Reference SILC Crypto Library Introduction to SILC RNG SILC RNG Interface SILC Cipher API SILC PKCS API SILC Hash Interface SILC HMAC Interface Resource Links SILC Project Website SILC Protocol Documentation SILC White Paper SILC FAQ
SilcCommandFlags NAME
        typedef enum { ... } SilcCommandFlags;
DESCRIPTION
        Command flags that set how the commands behave on different
        situations. These can be OR'es together to set multiple flags.
        The application is resoponsible of implementing the behaviour
        of these flags. These are here just to define generic flags.
        The server usually makes use of these flags.
SOURCE
        typedef enum {
          SILC_CF_NONE           = 0,

          /* Command may only be used once per (about) 2 seconds. Bursts up
             to 5 commands are allowed though. */
          SILC_CF_LAG            = (1L << 1),

          /* Command may only be used once per (about) 2 seconds. No bursts
             are allowed at all. */
          SILC_CF_LAG_STRICT     = (1L << 2),

          /* Command is available for registered connections (connections
             whose ID has been created. */
          SILC_CF_REG            = (1L << 3),

          /* Command is available only for server operators */
          SILC_CF_OPER           = (1L << 4),

          /* Command is available only for SILC (router) operators. If this
             is set SILC_CF_OPER is not necessary to be set. */
          SILC_CF_SILC_OPER      = (1L << 5),

        } SilcCommandFlag;
SILC Command Interface SilcCommandCb SilcCommandPayload SilcCommandFlags SilcCommand silc_command_payload_parse silc_command_payload_encode silc_command_payload_encode_payload silc_command_payload_encode_va silc_command_payload_encode_vap silc_command_reply_payload_encode_va silc_command_reply_payload_encode_vap silc_command_free silc_command_get silc_command_get_args silc_command_get_ident silc_command_get_status silc_command_set_ident silc_command_set_command

Copyright © 2001 - 2002 SILC Project SILC Project Website | SILC Toolkit Reference Manual Index