Copyright © 2001 - 2002 SILC Project SILC Project Website | SILC Toolkit Reference Manual

SILC Toolkit Reference Manual SILC Core Library SILC Authentication Interface SILC Channel Interface SILC Command Interface SILC Notify Interface SILC Status Types SILC Modes SILC ID Interface SILC ID Cache Interface SILC Argument Interface SILC Private Message Interface Packet Protocol Interface SILC Math Library SILC MP Interface SILC Math Interface SILC SFTP Library SILC SFTP Interface SFTP Filesystems Interface SILC Utility Library Basic SILC Types SILC Buffer Interface SILC Buffer Format Interface SILC Hash Table Interface SILC Logging Interface SILC Memory Interface SILC Mutex Interface SILC Thread Interface SILC Network Interface SILC Schedule Interface SILC Socket Interface SILC Protocol Interface SILC Config Interface SILC File Util Interface SILC String Util Interface SILC Util Interface SILC List Interface SILC Dynamic List Interface SILC Zip API SILC Key Exchange Library SILC SKE Interface SKE Status Types SKE Diffie Hellman Groups SKE Payloads SILC Client Library Using SILC Client Library Client Library Interface SILC Crypto Library Introduction to SILC RNG SILC RNG Interface SILC HMAC Interface SILC Cipher API SILC Hash API SILC PKCS API Resource Links SILC Project Website SILC Protocol Documentation SILC White Paper SILC FAQ
Function silc_command_reply_payload_encode_va SYNOPSIS
        SilcBuffer
        silc_command_reply_payload_encode_va(SilcCommand cmd,
                                             SilcStatus status,
                                             SilcStatus error,
                                             SilcUInt16 ident,
                                             SilcUInt32 argc, ...);
DESCRIPTION
        Same as silc_command_payload_encode_va except that this is used to
        encode strictly command reply packets.  The `argc' must not count
        `status' and `error' as arguments.  The `status' includes the
        command reply status.  If single reply will be sent then it includes
        SILC_STATUS_OK if error did not occur.  It includes an error value
        if error did occur.  In this case `error' field is ignored.  If
        there will be multiple successful command replies then the `status'
        includes a list value and `error' is ignored.  If there will
        multiple error replies the `status' includes a list value, and
        the `error' includes an error value.  Thus, the `error' value is
        specified only if there will be list of errors.
NOTES
        Protocol defines that it is possible to send both list of successful
        and list of error replies at the same time, as long as the error
        replies are sent after the successful replies.
SILC Command Interface SilcCommandCb SilcCommandPayload SilcCommandFlags SilcCommand silc_command_payload_parse silc_command_payload_encode silc_command_payload_encode_payload silc_command_payload_encode_va silc_command_payload_encode_vap silc_command_reply_payload_encode_va silc_command_reply_payload_encode_vap silc_command_free silc_command_get silc_command_get_args silc_command_get_ident silc_command_get_status silc_command_set_ident silc_command_set_command

Copyright © 2001 - 2002 SILC Project SILC Project Website | SILC Toolkit Reference Manual