Main Page Modules Data Structures File List Data Fields Globals Related Pages

# bpf_stat Struct Reference
[Packet.dll definitions and data structures]

Structure that contains a couple of statistics values on the current capture. More...

`#include <Packet32.h>`

## Data Fields
UINT | bs_recv
UINT | bs_drop
UINT | ps_ifdrop
| drops by interface. XXX not yet supported
UINT | bs_capt

## Detailed Description

Structure that contains a couple of statistics values on the current capture.

It is used by packet.dll to return statistics about a capture session.

Definition at line 145 of file Packet32.h.

## Field Documentation

UINT bs_capt

| number of packets that pass the filter, find place in the kernel buffer and thus reach the application. Definition at line 153 of file Packet32.h. Referenced by PacketGetStatsEx().

UINT bs_drop

| number of packets that the driver lost from the beginning of a capture. Basically, a packet is lost when the the buffer of the driver is full. In this situation the packet cannot be stored and the driver rejects it. Definition at line 149 of file Packet32.h. Referenced by main(), PacketGetStats(), and PacketGetStatsEx().

UINT bs_recv

| Number of packets that the driver received from the network adapter from the beginning of the current capture. This value includes the packets lost by the driver. Definition at line 146 of file Packet32.h. Referenced by main(), PacketGetStats(), and PacketGetStatsEx().

UINT ps_ifdrop

| drops by interface. XXX not yet supported Definition at line 152 of file Packet32.h. Referenced by PacketGetStatsEx().

The documentation for this struct was generated from the following file:

- Packet32.h

documentation. Copyright (c) 2002-2003 Politecnico di Torino. All rights reserved.