Main Page | Modules | Data Structures | File List | Data Fields | Globals | Related Pages

# PacketHeader Struct Reference
[NPF structures and definitions]

Structure prepended to each packet in the kernel buffer pool. More...

`#include <Packet.h>`

## Data Fields
ULONG | SN
| Sequence number of the packet.
bpf_hdr | header
| bpf header, created by the tap, and copied unmodified to user level programs.

## Detailed Description

Structure prepended to each packet in the kernel buffer pool.

Each packet in one of the kernel buffers is prepended by this header. It encapsulates the bpf_header, which will be passed to user level programs, as well as the sequence number of the packet, set by the producer (the tap function), and used by the consumer (the read function) to "reorder" the packets contained in the various kernel buffers.

Definition at line 399 of file Packet.h.

## Field Documentation

struct bpf_hdr header

| bpf header, created by the tap, and copied unmodified to user level programs. Definition at line 402 of file Packet.h. Referenced by NPF_tap().

ULONG SN

| Sequence number of the packet. Definition at line 401 of file Packet.h.

The documentation for this struct was generated from the following file:

- Packet.h

documentation. Copyright (c) 2002-2003 Politecnico di Torino. All rights reserved.